### Twister T2 Trimmer (TWISTER-T2)

|  |  |
| --- | --- |
| Input Voltage | 120V |
| Current Draw | 14.8A |
| Blade Motor | 1HP, Fan Cooled, Stainless |
| Tumbler Motor | 1/30HP, Epoxy Coated, Watertight |
| Cut Height | .040in |
| Weight | 215lbs |
| Shipping Weight (complete w/leaf collector) | 420lbs |
| Length | 42.5in |
| Width, with wheels | 27.5in |
| Width, without wheels | 20.5in |
| Height | 32.5in |
| Height without wheels | 30.5in |
| Discharge | 6in |